스피커 KT-182W  규격서

1) 기 능

KT-182W는 18인치 Neodymium driver를 채용한 1200W 고출력 서브우퍼 시스템입니다. 최고 수준의 고품질 부품을 채택하여 맑고, 풍부하며 선명한 원음을 재생하여 콘서트홀, 락 밴드 등의 공연에 적합하도록 강력한 저음 전달력을 제공합니다.

다양한 현장에서 다양한 용도로 사용될 수 있도록 통합된 3개의 fly track이 제공되고 내구성이 우수한 Neutrik NL4 Connector를 사용하여 제품 신뢰성이 우수한 중대형급 서브우퍼 시스템입니다.

Poly Urea 코팅 인클로저 마감 기술은 높은 인장 강도, 방수성, 견고함을 제공하여 흠집 및 파손이 빈번한 투어링 시스템에 외장 마감으로는 높은 내구성을 제공합니다. Neutrik NL4 connector, PLYING KIT이 포함되어 사용자 편의성을 높였습니다.

2) 특 징

Single 18" LF driver with exceptional intelligibility and high SPL output

High peak power yields excellent transient reproduction

Extremely low distortion for ultimate low-frequency clarity

Poly Urea Coating (KOREAN Patent) for scratch resistance

Arrayable in blocks to attain very high SPL with long throw

Easy and Convenient Rigging Tools : Integrated splay brackets

13 fly birch fly wood enclosure

3) 규격 (Specification)

컴포넌트	1x18" Driver
음압 감도	136 dB
정격 출력	LF-1200W
주파수 범위	±2dB -32 Hz ~ 200 Hz
입력 단자	2x Neutrik NL4 Speakon
크기 (mm)	600 (H) x 750 (W) x 840 (D) mm
무게	53.6 kg
색상	Black